NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Thailand  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:** Thai Industrial Standards Institute (TISI), Ministry of Industry  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  WTO/TBT Enquiry Point and Notification Authority,  Thai Industrial Standards Institute (TISI), Ministry of Industry  Tel.: (662) 202 3504 Fax: (662) 202 3511 E-mail: [thaitbt@tisi.mail.go.th](mailto:thaitbt@tisi.mail.go.th)  Website: <http://www.tisi.go.th> |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****],** **5.7.1 [****],** **other****:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** 29.140.30 - Fluorescent lamps. Discharge lamps |
| **5.** | **Title, number of pages and language(s) of the notified document:** Draft Thai Industrial Standard for Self-Ballasted Lamps for General Lighting Services by Rated Voltage >50 V: Safety Requirements (TIS 2780-25XX (20XX)) (23 page(s), in Thai) |
| **6.** | **Description of content:** The Thai Industrial Standards Institute (TISI) has proposed the draft compulsory Thai industrial standard forself-ballasted lamps for general lighting services by rated voltage >50 V: safety requirements (TIS 2780-25xx (20xx)).  This standard specifies safety and inter-changeability requirements, together with the test methods and conditions, required to show compliance of LED-lamps with integrated means for controlling starting and stable operation (self-ballasted lamps), intended for domestic and similar general lighting purposes, having:  - a rated wattage up to 60 W;  - a rated voltage of > 50 V up to 250 V;  - caps according to Table 1  The requirements of this standard relate only to type testing.  Recommendations for whole product testing or batch testing are identical with IEC 62031 Annex C. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Protection of human health or safety |
| **8.** | **Relevant documents:**   * IEC 62560:2011+AMD1:2015 Self-ballasted LED-lamps for general lighting services by voltage >50 V - Safety specifications |
| **9.** | **Proposed date of adoption:** To be determined  **Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:**  WTO/TBT Enquiry Point and Notification Authority Thai Industrial Standards Institute Tel: (66 2) 202 3504 Fax: (66 2) 202 3511 E-mail: [thaitbt@tisi.mail.go.th](mailto:thaitbt@tisi.mail.go.th) Website: <http://www.tisi.go.th>  <https://members.wto.org/crnattachments/2019/TBT/THA/19_4258_00_x.pdf> |