NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Thailand **If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** Thai Industrial Standards Institute (TISI), Ministry of Industry**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** WTO/TBT Enquiry Point and Notification AuthorityThai Industrial Standards Institute (TISI), Ministry of Industry Tel.: (662) 430 6831 ext. 2130 Fax: (662) 354 3041E-mail: thaitbt@tisi.mail.go.thWebsite: <http://www.tisi.go.th> |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****],** **5.7.1 [****],** **other****:**  |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Hot-dip 55% aluminium/zinc-coated flat steel (ICS 77.140.50); Flat steel products and semi-products (ICS 77.140.50) |
| **5.** | **Title, number of pages and language(s) of the notified document:** Draft Ministerial Regulation on Hot-dip 55% aluminium/zinc-coated flat steel (TIS 2228-2565) (29 page(s), in Thai) |
| **6.** | **Description of content:** The draft ministerial regulation mandates hot-dip 55%aluminium/zinc-coated flat steel to conform with the standard for Hot-dip 55% aluminium/zinc-coated flat steel (TIS 2228-2565).This standard covers hot-dip flat steel with aluminium/zinc-coating mass not greater than 4.0 mm in thickness and 1 500 mm in wideness. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Protection of human health or safety |
| **8.** | **Relevant documents:** -    AS 1397-2011 Continuous hot-dip metallic coated steel sheet and strip – coatings of zinc and zinc alloyed with aluminium and magnesium-    AS/NZS 1365: 1996 Tolerances for flat-rolled steel products-    ISO 14284: 1996 Steel and iron – Sampling and preparation of samples for the determination of chemical composition-    ISO 17925: 2004 Zinc and/or aluminium based coatings on steel - Determination of coating mass per unit area and chemical composition - Gravimetry, inductively coupled plasma atomic emission spectrometry and flame atomic absorption spectrometry-    ISO 1460: 1992 Metallic coatings-Hot dip galvanized coatings on ferrous materials Gravimetric determination of the mass per unit area-    JIS G 0320: 2009 Standard test method for heat analysis of steel products-    JIS G 0320: 2009/ AMENDMENT 1: 2015 Standard test method for heat analysis of steel-    products (Amendment 1)-    JIS G 0320: 2009/ AMENDMENT 2: 2017 Standard test method for heat analysis of steel-    products (Amendment 2)-    JIS G 0321: 2017 Product analysis and its tolerance for wrought steel-    JIS G 0404: 2014 Steel and steel products – General technical delivery requirements-    JIS G 3321: 2019 Hot-dip 55% aluminium-zinc alloy-coated steel sheet and strip-    JIS Z 8401: 2019 Rounding of numbers-   TIS 2172 - Part 1-2556 Metallic materials - tensile testing - part 1 : method of test at room temperature |
| **9.** | **Proposed date of adoption:** To be determined**Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [** **]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:** WTO/TBT Enquiry Point and Notification AuthorityThai Industrial Standards Institute (TISI), Ministry of Industry Tel.: (662) 430 6831 ext. 2130 Fax: (662) 354 3041E-mail: thaitbt@tisi.mail.go.thWebsite: <http://www.tisi.go.th><https://members.wto.org/crnattachments/2022/TBT/THA/22_2039_00_x.pdf> |